# FreeDATA - DAEMON network documentation 


## GET DAEMON STATE
#### Description:
Get the current daemon state

#### Parameters
- Type: GET 
- Command: DAEMON_STATE
- Parameter: --- (str)

#### Example 
```
{"type" : "GET", "command" : "DAEMON_STATE"}
```

#### Returns
```
{
	"COMMAND": "DAEMON_STATE",
	"DAEMON_STATE": [],
	"PYTHON_VERSION": str(python_version),
	"HAMLIB_VERSION": str(hamlib_version),
	"INPUT_DEVICES": [],
	"OUTPUT_DEVICES": [],
	"SERIAL_DEVICES": [], 
	"CPU": "", 
	"RAM": "", 
	"VERSION": "0.1-prototype"
}
```


## SET CALLSIGN
#### Description:
Save your callsign to the daemon

#### Parameters
- Type: SET 
- Command: MYCALLSIGN
- Parameter: callsign (str)
- timestamp: unix timestamp (str)

#### Example 
```
{"type" : "SET", "command": "MYCALLSIGN" , "parameter": "<callsign>", "timestamp" : "123456789"}
```



## SET GRIDSQUARE
#### Description:
Save your gridsquare/maidenhead-locator to the daemon

#### Parameters
- Type: SET 
- Command: MYGRID
- Parameter: gridsquare (str)
- timestamp: unix timestamp (str)

#### Example 
```
{"type" : "SET", "command": "MYGRID" , "parameter": "<gridsquare>", "timestamp" : "123456789"}
```



## TEST HAMLIB
#### Description:
Test your hamlib settings

#### Parameters
- Type: GET 
- Command: TEST_HAMLIB
- Parameter: obj
	- devicename
	- deviceport
	- pttprotocol
	- pttport
	- serialspeed
	- data_bits
	- stop_bits
	- handshake
- timestamp: unix timestamp (str)

#### Example 
```
{
        "type": "GET",
        "command" : "TEST_HAMLIB",
        "parameter" : [{
            "devicename" : "<devicename>",
            "deviceport" : "<deviceport>",
            "pttprotocol" : "<pttprotocol>",
            "pttport" : "<pttport>",
            "serialspeed" : "<serialspeed>",
            "data_bits" : "<data_bits>",
            "stop_bits" : "<stop_bits>",
            "handshake" : "<handshake>"
        }]
    }
```


## START TNC
#### Description:
Start the tnc process

#### Parameters
- Type: GET 
- Command: TEST_HAMLIB
- Parameter: obj
	- mycall
	- mygrid
	- rx_audio
	- tx_audio
	- devicename
	- deviceport
	- pttprotocol
	- pttport
	- serialspeed
	- data_bits
	- stop_bits
	- handshake

#### Example 
```
{
        type: 'SET',
        command: 'STARTTNC',
        parameter: [{
            mycall: mycall,
            mygrid: mygrid,
            rx_audio: rx_audio,
            tx_audio: tx_audio,
            devicename: devicename,
            deviceport: deviceport,
            pttprotocol: pttprotocol,
            pttport: pttport,
            serialspeed: serialspeed,
            data_bits: data_bits,
            stop_bits: stop_bits,
            handshake: handshake

        }]
    }
```

## STOP TNC
#### Description:
Stop the tnc process

#### Parameters
- Type: SET 
- Command: STOPTNC
- Parameter: ---

#### Example 
```
{"type" : "SET", "command": "STOPTNC" , "parameter": "---" }
```




    
    
    
    
