# Override some defaults so BT stack is enabled
# by default in this example
CONFIG_BT_ENABLED=y
CONFIG_BTDM_CTRL_MODE_BLE_ONLY=y
CONFIG_BTDM_CTRL_MODE_BR_EDR_ONLY=n
CONFIG_BTDM_CTRL_MODE_BTDM=n
CONFIG_BTDM_MODEM_SLEEP=n
CONFIG_BTDM_BLE_SCAN_DUPL=y
CONFIG_BTDM_SCAN_DUPL_TYPE=2
CONFIG_BTDM_SCAN_DUPL_TYPE_DATA_DEVICE=y
CONFIG_BTDM_SCAN_DUPL_CACHE_SIZE=200
CONFIG_BTDM_BLE_MESH_SCAN_DUPL_EN=y
CONFIG_BTDM_MESH_DUPL_SCAN_CACHE_SIZE=200
CONFIG_BTDM_CTRL_FULL_SCAN_SUPPORTED=y
CONFIG_BTDM_BLE_ADV_REPORT_FLOW_CTRL_SUPP=y
CONFIG_BLE_MESH=y
CONFIG_BLE_MESH_HCI_5_0=y
CONFIG_BLE_MESH_USE_DUPLICATE_SCAN=y
CONFIG_BLE_MESH_PROV=y
CONFIG_BLE_MESH_PROVISIONER=y
CONFIG_BLE_MESH_WAIT_FOR_PROV_MAX_DEV_NUM=10
CONFIG_BLE_MESH_MAX_PROV_NODES=10
CONFIG_BLE_MESH_MAX_STORED_NODES=10
CONFIG_BLE_MESH_PBA_SAME_TIME=1
CONFIG_BLE_MESH_PBG_SAME_TIME=1
CONFIG_BLE_MESH_PROVISIONER_SUBNET_COUNT=3
CONFIG_BLE_MESH_PROVISIONER_APP_KEY_COUNT=3
CONFIG_BLE_MESH_PB_ADV=y
CONFIG_BLE_MESH_NET_BUF_POOL_USAGE=y
CONFIG_BLE_MESH_PB_GATT=y
CONFIG_BLE_MESH_GATT_PROXY_SERVER=n
CONFIG_BLE_MESH_RELAY=y
CONFIG_BLE_MESH_LOW_POWER=n
CONFIG_BLE_MESH_FRIEND=n
CONFIG_BT_BTU_TASK_STACK_SIZE=4512
CONFIG_BLE_MESH_CFG_CLI=y
CONFIG_BLE_MESH_GENERIC_ONOFF_CLI=y
CONFIG_BLE_MESH_ADV_BUF_COUNT=100
CONFIG_BLE_MESH_CRPL=10
CONFIG_BLE_MESH_TX_SEG_MSG_COUNT=10
CONFIG_BLE_MESH_RX_SEG_MSG_COUNT=10
CONFIG_BLE_MESH_RX_SDU_MAX=384
CONFIG_BLE_MESH_TX_SEG_MAX=32
CONFIG_BLE_MESH_NO_LOG=n
CONFIG_BLE_MESH_STACK_TRACE_LEVEL=1
