# Override some defaults so BT stack is enabled
# by default in this example
CONFIG_BT_ENABLED=y
CONFIG_BTDM_CTRL_MODE_BLE_ONLY=y
CONFIG_BTDM_CTRL_MODE_BR_EDR_ONLY=n
CONFIG_BTDM_CTRL_MODE_BTDM=n
CONFIG_BTDM_MODEM_SLEEP=n
CONFIG_BTDM_BLE_SCAN_DUPL=y
CONFIG_BTDM_SCAN_DUPL_TYPE=2
CONFIG_BTDM_SCAN_DUPL_TYPE_DATA_DEVICE=y
CONFIG_BTDM_SCAN_DUPL_CACHE_SIZE=200
CONFIG_BTDM_BLE_MESH_SCAN_DUPL_EN=y
CONFIG_BTDM_MESH_DUPL_SCAN_CACHE_SIZE=200
CONFIG_BTDM_CTRL_FULL_SCAN_SUPPORTED=y
CONFIG_BTDM_BLE_ADV_REPORT_FLOW_CTRL_SUPP=y
CONFIG_BT_GATTS_ENABLE=y
CONFIG_BT_GATTS_SEND_SERVICE_CHANGE_MANUAL=y
CONFIG_BLE_MESH=y
CONFIG_BLE_MESH_HCI_5_0=y
CONFIG_BLE_MESH_USE_DUPLICATE_SCAN=y
CONFIG_BLE_MESH_NODE=y
CONFIG_BLE_MESH_PROV=y
CONFIG_BLE_MESH_NET_BUF_POOL_USAGE=y
CONFIG_BLE_MESH_PROXY=y
CONFIG_BLE_MESH_PB_GATT=y
CONFIG_BLE_MESH_GATT_PROXY_SERVER=y
CONFIG_BLE_MESH_NODE_ID_TIMEOUT=60
CONFIG_BLE_MESH_PROXY_FILTER_SIZE=1
CONFIG_BLE_MESH_SUBNET_COUNT=1
CONFIG_BLE_MESH_APP_KEY_COUNT=1
CONFIG_BLE_MESH_MODEL_KEY_COUNT=1
CONFIG_BLE_MESH_MODEL_GROUP_COUNT=1
CONFIG_BLE_MESH_LABEL_COUNT=1
CONFIG_BLE_MESH_CRPL=10
CONFIG_BLE_MESH_MSG_CACHE_SIZE=10
CONFIG_BLE_MESH_ADV_BUF_COUNT=60
CONFIG_BLE_MESH_TX_SEG_MSG_COUNT=6
CONFIG_BLE_MESH_RX_SEG_MSG_COUNT=1
CONFIG_BLE_MESH_RX_SDU_MAX=384
CONFIG_BLE_MESH_TX_SEG_MAX=32
CONFIG_BLE_MESH_RELAY=y
CONFIG_BLE_MESH_LOW_POWER=n
CONFIG_BLE_MESH_FRIEND=n
CONFIG_BLE_MESH_CFG_CLI=y
CONFIG_BT_BTU_TASK_STACK_SIZE=4512
